{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":39,"n_cols":5,"rows_kept":39,"cut":false,"hidden":false,"merged":[[2,0,2,4],[33,0,33,4],[37,0,37,1],[37,2,37,4],[38,0,38,1],[38,2,38,4],[40,1,40,3],[0,0,1,4]],"flags":["formulas_cached_only"]}
["研发设计原始BOM表\n（电子部分）"]
[]
["AiPi-Voice_V1.0 (外挂8388语音芯片)"]
["元件料号","规           格","单位","用量","贴片位置"]
[11277001,"贴片电容-0402-X5R-8.2PF±10%-16V","PCS",1,"C78"]
[11105001,"贴片电容-0402-NP0/C0G-47PF±5%-50V","PCS",6,"C49,C50,C51,C57,C58,C59"]
[11104023,"贴片电容-0402-NP0/C0G-100PF±5%-16V","PCS",2,"C48,C56"]
[11031003,"贴片电容-0402-X5R-0.1UF±10%-16V","PCS",14,"C3,C4,C18,C23,C27,C31,C38,C40,C42,C46,C54,C63,C68,C82"]
[11050002,"贴片电容-0402-X5R-0.47uF-±10%-10V-编带","PCS",2,"C61,C66"]
[11031002,"贴片电容-0402-X5R-1UF±10%-16V","PCS",8,"C34,C35,C36,C37,C60,C65,C70,C71"]
[11120003,"贴片电容-0603-X5R-10UF±10%-10V","PCS",18,"C5,C6,C17,C20,C21,C24,C25,C28,C30,C32,C39,C41,C43,C47,C55,C64,C69,C81"]
[10021008,"贴片电阻-0402-0R-±5%-1/16W","PCS",8,"R1,R2,R35,R53,C44,C45,C52,C53"]
[10041012,"贴片电阻-0603-0R ±5%-1/10W","PCS",5,"R12,R16,R18,R29,R56"]
[10021014,"贴片电阻-0402-10R-±5%-1/16W","PCS",1,"R24"]
[10021026,"贴片电阻-0402-33R±5%-1/16W","PCS",3,"R19,R21,R57"]
[10021006,"贴片电阻-0402-1K-±5%-1/16W","PCS",10,"R58,R59,R60,R61,R62,R63,R64,R65,R66,R67"]
[10021035,"贴片电阻-0402-2.2K-±5%-1/16W","PCS",2,"R54,R55"]
[10021010,"贴片电阻-0402-5.1K-±5%-1/16W","PCS",2,"R17,R20"]
[10021034,"贴片电阻-0402-10K±5%-1/16W","PCS",2,"R68,R71"]
[10021007,"贴片电阻-0402-30K-±5%-1/16W","PCS",2,"R69,R72"]
[10011010,"贴片电阻-0402-110K-±1%-1/16W","PCS",1,"R10"]
[10011025,"贴片电阻-0402-150K-±1%-1/16W","PCS",2,"R70,R73"]
[10011009,"贴片电阻-0402-510K±1%-1/16W","PCS",1,"R7"]
[15025002,"ESD保护器件-0402-PESD0402V05P03","PCS",3,"D4,D5,D6"]
[22061003,"USB母座-TYPE-C-16Pin-8.94*7.35*4.3mm-编带","PCS",1,"USB2"]
[12120001,"贴片电感-3015-2.2UH±20%","PCS",1,"L1"]
[17010004,"按钮开关-贴片按键 轻触开关 微动开关 3*4*2MM-编带包装","PCS",2,"S1,S2"]
[22010218,"卧式贴片插座-1*2PIN-1.25mm间距-针座-米黄色-超薄-编带","PCS",4,"J1,J2,J5,J6"]
[19033001,"电源芯片-RICHTEK-RT8059-3.3V/1A-SOT23-5","PCS",1,"U5"]
[19050105,"音频解码芯片-顺芯-ES8388-QFN28-4*4mm-编带","PCS",1,"U6"]
[19054127,"功放IC-英锐芯（IDCHIP）-8002D-SOP8-编带","PCS",2,"U3,U11"]
[90380008,"Ai-M61-32S_V1.1-IO引脚全引出-2128号Combo常规固件-丝印待定-接入板载天线-无其它要求-编带","PCS",1,"U1"]
[null,"PCB板-AiPi-Voice&Audio_V1.0-双面板-黑油-白字-OSP-覆盖塞孔-95*136*1.0mm-2*2pcs","PCS",1]
["DIP"]
[22070162,"单排排针-黑色直针-2.54mm间距1*10PIN-下针长3.0mm-上针长6.0mm-塑高2.54mm","PCS",3,"J4,J7,J8"]
[22010220,"咪头-7232-接收灵敏度-65dB-2PIN-1.25mm间距-交叉绞线长100mm-红正-黑负-米黄色超薄插头-静电袋","PCS",2]
[16010095,"腔体喇叭-线长100mm-8R2W-L53*W18*H9mm-带2PIN间距1.25mm米黄色超薄插头-袋装","PCS",2]
["研发部：袁南南  2023年06月27日",null,"制造工程："]
["产品工程：",null,"接收部门："]